	Tipul de material
	Continut (% din masa totala)
	Masa materialului din componenta computerului (kg)
	Unde este folosit
	Localizare

	Plastic

	22.9907

	6.26

	Insulation

	Cable, Housing


	Plumb

	6.2988

	1.72

	Metal joining

	Funnel glass in CRTs, PWB


	Aluminiu

	14.1723

	3.86

	Structural, Conductivity

	Housing, CRT, PWB, connectors


	Germaniu

	0.0016

	< 0.1

	Semiconductor

	PWBs


	Galliu

	0.0013

	< 0.1

	Semiconductor

	PWBs


	Fier

	20.4712

	5.58

	Structural, Magnetivity

	Housing,CRTs, PWBs


	Cositor

	1.0078

	0.27

	Metal joining

	PWBs, CRTs


	Cupru

	6.9287

	1.91

	Conductivity

	CRTs, PWBs, connectors


	Bariu

	0.0315

	< 0.1

		Panel glass in CRTs


	Nickel

	0.8503

	0.23

	Structural, Magnetivity

	Housing, CRT, PWB


	Zinc

	2.2046

	0.6

	Battery, Phosphor emitter

	PWB, CRT


	Tantalum

	0.0157

	< 0.1

	Capacitor

	Capacitors/PWB, power supply


	Indium

	0.0016

	< 0.1

	Transistor, rectifier

	PWB


	Vanadiu

	0.0002

	< 0.1

	Red Phosphor emitter

	CRT


	Terbiu

	0

	0

	Green phosphor activator, dopant

	CRT, PWB


	Berylliu

	0.0157

	< 0.1

	Thermal Conductivity

	PWB, connectors


	Aur 

	0.0016

	< 0.1

	Connectivity, Conductivity

	Connectivity, conductivity/PWB, connectors


	Europium

	0.0002

	< 0.1

	Phosphor activator

	PWB


	Titanium

	0.0157

	< 0.1

	Pigment, alloying agent

	Housing


	Ruthenium

	0.0016

	< 0.1

	Resistive circuit

	PWB


	Cobalt

	0.0157

	< 0.1

	Structural, Magnetivity

	Housing, CRT, PWB


	Palladium

	0.0003

	< 0.1

	Connectivity, Conductivity

	PWB, connectors


	Manganese

	0.0315

	< 0.1

	Structural, Magnetivity

	Housing, CRT, PWB


	Argint

	0.0189

	< 0.1

	Conductivity

	Conductivity/PWB, connectors


	Antimoniu

	0.0094

	< 0.1

	Diodes

	Housing, PWB, CRT


	Bismuth

	0.0063

	< 0.1

	Wetting agent in thick film

	PWB


	Chromium

	0.0063

	< 0.1

	Decorative, Hardner

	Housing


	Cadmium

	0.0094

	< 0.1

	Battery, blue-green Phosphor emitter

	Housing, PWB, CRT


	Selenium

	0.0016

	0.00044

	Rectifiers

	rectifiers/PWB


	Niobium

	0.0002

	< 0.1

	Welding

	Housing


	Yttrium

	0.0002

	< 0.1

	Red Phosphor emitter

	CRT


	Rhodium

	0

	 

	Thick film conductor

	PWB


	Platinum

	0

	 

	Thick film conductor

	PWB


	Mercur

	0.0022

	< 0.1

	Batteries, switches

	Housing, PWB


	Arsenic

	0.0013

	< 0.1

	Doping agent in transistors

	PWB


	Silica

	24.8803

	6.8

	Glass, solid state devices

	CRT,PWB



	
 
Sursa: Microelectronics and Computer Technology Corporation (MCC). 1996.
Electronics Industry Environmental Roadmap. Austin, TX: MCC. 
	[image: image1.png]




	[image: image2.png]



	[image: image3.png]





